# PRILOG B/*ANNEX B*

**TEHNIČKE SPECIFIKACIJE (za nabavu robe)/ TECHNICAL SPECIFICATIONS**

Naziv Naručitelja/the Contracting Authority: POBIS društvo s ograničenom odgovornošću za trgovinu i usluge

Adresa/Address: Dravska ulica 16 , 48000 Koprivnica OIB / Identification / Registration Number: 86536126262

Kontakt broj mobilnog telefona / Mobile phone contact number: +385 98 452 905

Predmet nabave je nabava „skiving“ mašine za pripremu spoja na brusnim trakama s dodatkom za prešanje uskih i širokih traka / The subject of procurement is procurement of „skiving“ machine for the preparation of joints on abrasive belts with the addition for pressing narrow and wide belts

Interni evidencijski broj nabave: 001/2021

Internal reference number of procurement: 001/2021

NAPOMENA:

Ponuditelj obavezno popunjava stupac „Ponuđene specifikacije“ definirajući detaljno tehničke specifikacije ponuđene robe (**napomena**: ponuditelj popunjava tehničke specifikacije upisujući točne karakteristike ponuđene robe, izbjegavajući pri tome popunjavanje stupca samo riječima kao što su npr. „zadovoljava“, „DA“, „jednakovrijedno traženom“ ili „odgovara“. Ukoliko ponuditelj ne upiše točne karakteristike ponuđene robe njegova ponuda može biti odbačena). / The tenderer must fill in the "Specifications Offered" column by defining in detail the technical specifications of the goods offered (note: the tenderer fills in the technical specifications by entering the exact characteristics of the goods offered, avoiding filling the column only with words such as "meets", "yes", "equivalent to the requested" or "fits". If the tenderer does not enter the exact characteristics of the offered goods, his offer may be rejected).

Stupac „Napomene, reference na ponudu“ ponuditelj može popuniti ukoliko smatra potrebnim. Stupac „Ocjena Odbora za nabavu DA/NE“ ponuditelj **ne popunjava** s obzirom na to da je stupac predviđen za ocjene naručitelja. / The "Notes, References" column can be filled in by the tenderer if he finds it necessary. The "yes/no Procurement Committee Rating" column is not filled in by the tenderer as the column is provided for the contracting entity's assessments.

Zahtjevi definirani Tehničkim specifikacijama predstavljaju minimalne tehničke karakteristike koje ponuđena roba mora zadovoljavati, ukoliko nije drugačije navedeno, te ih ponuditelji ne smiju mijenjati. /The requirements defined by the Technical Specifications represent the minimum technical characteristics that the goods offered must meet, unless otherwise stated, and may not be changed by the tenderers.

Za svaku naznaku robne marke uz koju nije naznačena mogućnost nuđenja jednakovrijedne robe, za potrebe ove Dokumentacije o nabavi uzima se da uz istu stoje riječi ‘’ili jednakovrijedno’’ te je ponuditelju dopušteno ponuditi robu koja je jednakovrijedna./ For any indication of a brand that does not indicate the possibility of offering equivalent goods, for the purposes of this Procurement Documentation it shall be taken that the words "or equivalent" stand with it and the tenderer shall be allowed to offer goods that are equivalent.

|  |  |  |  |
| --- | --- | --- | --- |
| Tražene specifikacije/ Required specifications | Ponuđene specifikacije/ Specifications Offered | Napomene/Notes | Ocjena (da/ne)/Rating (yes/no) |
| Snaga: najmanje 10 kW / Power: at least 10 kW |  |  |  |
| Dijamantna glava za pripremu spoja „gruba“/  Diamond head with coarse diamond wheel |  |  |  |
| Dijamantna glava za pripremu spoja „fina“ / Diamond head with fine diamond wheel |  |  |  |
| Kontinuirani posmak/ Continous feeding |  |  |  |
| Automatsko brusenje i lijepljenje / Auto skiving, auto gluing |  |  |  |
| Glava s paralelnim brušenjem/ Head with parallel grinding |  |  |  |
| Glava s brušenjem pod 45°/ Head with grinding under 45° |  |  |  |
| Glava za četkanje s žičanom četkom/ Head for brushing with wire brush |  |  |  |
| Glava s clean&streap diskom/ Head with clean&streap disk |  |  |  |
| Glava za nanošenje lijepila/ One head for glue application |  |  |  |
| Glava za sušenje/ One head for drying |  |  |  |
| Dodatak za prešanje uskih brusnih traka do 400 mm širine/ Addition for pressing narrow abrasive belts up to 400 mm wide |  |  |  |
| Dodatak za prešanje širokih brusnih traka do 1900mm širine/ Addition for pressing wide abrasive belts up to 1900mm wide |  |  |  |
| Dostupni svi rezervni i habajući dijelovi za nesmetano korištenje u svo vrijeme eksploatacije stroja/ All spare and wear parts are available for unhindered use at all times of machine operation |  |  |  |
| Garancija - minimalno godinu dana/ Guarantee - for a minimum of one year |  |  |  |
| Tehnička podrška telefonski ili putem e-maila u roku od 24 sata  Technical support by telephone or e-mail within 24 hours |  |  |  |
| CE-norme / CE standards |  |  |  |
| Dokumentacija i tekst upravljanja je dostupna online na engleskom ili hrvatskom jeziku / Documentation and users guide is available online in Croatian or in English |  |  |  |
| Isporuka u Hrvatsku (do Naručitelja ili do najbliže luke) / Delivery to Croatia (to the Contracting authority or to the nearest port |  |  |  |
| Plaćanje: \_\_\_\_% avans, \_\_\_\_% prilikom isporuke / Payment: \_\_\_\_% advance, \_\_\_\_% by delivery |  |  |  |

U/*In* \_\_\_\_\_\_\_\_\_\_\_\_\_\_dana/*date*\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

ime, prezime, potpis ovlaštene osobe/

name, surname, signature of authorised person